Operational Scenarios
Case I: Undervoltage Feeder Sag Heavy loading profile drives N18 voltage down to 0.9290 p.u. Optimization maps dynamic shunt support.
Case II: Overvoltage Surge Condition Light load drives tail bus N33 up to 1.0627 p.u. Triggers distributed inductive reactor loops.
Case III: Coordinated OLTC Loop Corrects upstream overvoltage with Reactor N6 and addresses residual downstream sags via N12-N13 transformer tap adjustment.
Asset Dispatch Matrix
Cap N10
Cap N24
Cap N30
Reactor N6
Reactor N28
Reactor N32
OLTC Tap (N12-N13) 1.000 p.u.
Iterating MO-FGO Core Loop...
[21:10:16][SYSTEM] EnVVARCO Core initialized within 'grid-ops' namespace. Mapping 33-Bus topology frameworks... Ready.